
**T.C.**

**FATİH SULTAN MEHMET VAKIF UNIVERSTY FACULTY OF ENGINEERING**

****

## Fully Entegrated Intelligent Charge

## Estimation System


**UNDERGRADUATE GRADUATION PROJECT (END OF THE TERM REPORT)**

### Muhammed Eset TEPELER

**ELECTRIC-ELECTRONIC ENGINEERING DEPARTMENT**

**T.C.**

**FATİH SULTAN MEHMET VAKIF UNIVERSTY FACULTY OF ENGINEERING**

****

## Fully Entegrated Intelligent Charge

## Estimation System

**UNDERGRADUATE GRADUATION PROJECT (END OF THE TERM REPORT)**

**Muhammed Eset TEPELER  
2121241010**

**Advisor: Prof. Dr. Hilmi ÜNLÜ**

**Date Delivered to the Department:**

**ELECTRIC-ELECTRONIC ENGINEERING DEPARTMENT**

## Preface

People are constantly improving new technologies and completely integrating modern devices into new parts of everyday life. This underlined fact means that the demand for smart technologies that improve productivity, reliability, and Eco-friendliness will only continue to grow. The Fully Integrated Intelligent Charge Estimation System (FICES) project is an energy management solution that seeks to address current and emerging trends for managing energy in mobile applications such as battery-powered systems and electric vehicles.

The project focuses on creating an intelligent and self-adjusting structure that combines sophisticated algorithms with real-time data analysis to provide accurate charge level estimations. Unlike conventional methods of charge estimation which rely on simplistic measurements and static models, this system incorporates machine learning along with sensor fusion to provide context-aware estimation of charge with precision. These capabilities make performance optimization, battery longevity, and user trust in advanced power systems possible.

The work presented here reflects an entire spectrum from the theoretical model to the practical prototype. It combined various aspects such as embedded systems, artificial intelligence, electrical engineering and much more. The result is not a prototype, but a prototype that can modularly and structurally be adjusted to fulfill varying requirements and thus expand its range of application.

My advisor, who guided me with his knowledge and experience during the process of carrying out this study, I would like to thank Prof. Dr. Hilmi ÜNLÜ. We would also like to express my gratitude to my family and friends who supported me throughout the process..

June 2025 Muhammed Eset TEPELER

## TABLE OF CONTENTS

**Sayfa**

[ABBREVIATIONS 6](#_TOC_250033)

[TABLE LIST 7](#_TOC_250032)

[SHAPE LIST 8](#_TOC_250031)

ABSTRACT 9

ÖZET 10

1. [INTRODUCTION 11](#_TOC_250030)
   1. [Purpose of this thesis 11](#_TOC_250029)
   2. [Literature Review 11](#_TOC_250028)
      1. [Traffic Analysis and Prediction Systems  11](#_TOC_250027)
      2. [Energy Comsumption Forecasting Models 12](#_TOC_250026)
      3. [Geolocation Services in Traffic Systems 13](#_TOC_250025)
      4. [Charging Station Management Systems 13](#_TOC_250024)
      5. [Machine Learning in Traffic and Energy Analysis 14](#_TOC_250023)
2. [THEORETICAL FRAMEWORK AND ANALYSES 14](#_TOC_250022)
   1. [Traffic Analysis System 14](#_TOC_250021)
      1. [System Architecture 15](#_TOC_250020)
      2. [Route Planning and Analysis 16](#_TOC_250019)
      3. [Traffic Density Analysis 17](#_TOC_250018)
      4. [Real-time Traffic Information Processing  18](#_TOC_250013)
   2. [Energy Prediction Model 19](#_TOC_250012)
      1. [Model Architecture and Components  20](#_TOC_250011)
      2. [Feature Engineering and Data Pre-processing 20](#_TOC_250010)
      3. Model Training and Validation 20
      4. Implamentation Challanges and Soluations 21
      5. Performance Metrics 21
   3. **Interface Design and Visualization Tools 21**
      1. Frontend Implementation 22
         1. User Interface Design 22
         2. Interactive Maps Integration 23
      2. Backend Services 24
         1. API Integration 24
         2. Data Processing Services 24
         3. Real-time Updates 24
      3. Security Implamentation 24
      4. Implamentation Challanges and Soluations 24
      5. System Performance Metrics 25
   4. [Charging Station Analysis 25](#_TOC_250009)
      1. [Station Location Analysis 25](#_TOC_250008)
      2. [Usage Pattern Analysis 26](#_TOC_250007)
      3. Route-based Station Planning 27
      4. Implamentation Challanges and Soluations 27
      5. Performance Metrics 28
3. **IMPLEMENTATION AND RESULTS**
   1. Interface Design and Visualizition Tools 28
      1. Stationn Location Analysis 28
      2. Interactive Mapping and Real Time Visual Layers 28
      3. Backend API and Data Flow 29
      4. Flow Security Infrastacture 29
      5. Performance Metrics 29
      6. User Experiance Evulation 29
   2. Charging Station Analysis and Optimization 30
      1. Spatial Location Optimization 30
      2. Usage Pattern Modeling 31
      3. Route-Based Infrastracture Planning 31
      4. Implemantation Challanges and Mitigations 32
      5. Measured Impact and Performance 32
4. **DISCUSSION**
   1. System Performance Evaluation 33
   2. Challenges and Solutions 34
   3. Future Improvements 34

[CONCLUSION VE RECOMMENDATIONS 35](#_TOC_250002)

[REFERANCES 38](#_TOC_250001)

[SHAPE REFERANCES 45](#_TOC_250000)

TABLE REFERANCES 46

## ABBREVIATIONS

|  |  |
| --- | --- |
| **API:** | Application Programming Interface |

|  |  |
| --- | --- |
| **AR:** | Augmented Reality |

|  |  |
| --- | --- |
| **CSRF:** | Cross-Site Request Forgery |

|  |  |
| --- | --- |
| **DBSCAN:** | Density-Based Spatial Clustering of Applications with Noise |

|  |  |
| --- | --- |
| **ETL:** | Extract, Transform, Load |

|  |  |
| --- | --- |
| **EV:** | Electric Vehicle |

|  |  |
| --- | --- |
| **GIS:** | Geographic Information System |

|  |  |
| --- | --- |
| **GPU:** | Graphics Processing Unit |

|  |  |
| --- | --- |
| **HCI:** | Human-Computer Interaction |

|  |  |
| --- | --- |
| **IQR:** | Interquartile Range |

|  |  |
| --- | --- |
| **JSON:** | JavaScript Object Notation |

|  |  |
| --- | --- |
| **KPI:** | Key Performance Indicator |

|  |  |
| --- | --- |
| **MAE:** | Mean Absolute Error |

|  |  |
| --- | --- |
| **ML:** | Machine Learning |

|  |  |
| --- | --- |
| **MFA:** | Multi-Factor Authentication |

|  |  |
| --- | --- |
| **OAuth2:** | Open Authorization 2.0 |

|  |  |
| --- | --- |
| **PCA:** | Principal Component Analysis |

|  |  |
| --- | --- |
| **R²:** | Coefficient of Determination |

|  |  |
| --- | --- |
| **RBAC:** | Role-Based Access Control |

|  |  |
| --- | --- |
| **Redis:** | Remote Dictionary Server (in-memory data structure store) |

|  |  |
| --- | --- |
| **RMSE:** | Root Mean Square Error |

|  |  |
| --- | --- |
| **RNN:** | Recurrent Neural Network |

|  |  |
| --- | --- |
| **SDK:** | Software Development Kit |

|  |  |
| --- | --- |
| **SLA:** | Service-Level Agreement |

|  |  |
| --- | --- |
| **SSE:** | Server-Sent Events |

|  |  |
| --- | --- |
| **UI:** | User Interface |

|  |  |
| --- | --- |
| **V2G:** | Vehicle-to-Grid |

|  |  |
| --- | --- |
| **WCAG:** | Web Content Accessibility Guidelines |

|  |  |
| --- | --- |
| **WebSocket:** | A communication protocol for real-time bidirectional interaction |

|  |  |
| --- | --- |
| **XGBoost:** | Extreme Gradient Boosting (a machine learning algorithm) |

## TABLE LIST

**PAGE**

**Table 1:** Implementation Challenges and Solutions 24

**Table 2:** System Performance Metrics 25

**Table 3:** Summary of Charging Station Usage Profiles by Region 26

**Table 4:** EV Route Simulation and Optimal Charging Point Overlay 27

**Table 5:** Performance Metrics 28

**Table 6:** Performance Evaulation 29

**Table 7:** User Experience Evualiton 29

**Table 8:** Summary of Charging Station Usage Profiles by Region 31

**Table 9:** Traffic Prediction Performance Metrics 31

**Table 10:** Challenges and Mitigations 32

**Table 11:** Model Performance Comparison for Energy Consumotion Forecasting 32

**Table 12:** Traffic Prediction Performance Over Different Time Horizons 33

## SHAPE LIST

**Sayfa**

**Shape 1:** Energy Consumption Forecasting Models. 12

**Shape 2:** Flowchart of input and references datasets, geocoding procedure and outputs. 14

**Shape 3:** Distribution Of Charge Stations By Cities. 15

**Shape 4:** Code Block For Charge Stations. 16

**Shape 5:** Part of the Code Block that analyse traffic density. 17

**Shape 6:** Part of the Code Block That Makes Real Time Analysis) . 17

**Shape 7:** Part of the Code Block That Makes Energy Prediction 19

**Shape 8:** EV Car Estimation System Files 20

**Shape 9:** Traffic Control System 20

**Shape 10:** Energy Prediction model architecture 21

**Shape 11:** Architecture of the Traffic Analyis System 21

**Shape 12:** Spation Distribution of Existing Charging Stations in Urban Areas. 23

**Shape 13:** EV Charging Station Analysis Framework. 23

**Shape 14:** Component Integration Architecture. 25

## FULLY ENTEGRATED INTELLIGENT CHARGE ESTIMATION SYSTEM

## ABSTRACT

The mass adoption of electric vehicles (EVs) has caused a necessity for the creation of smart and efficient charging station management systems on a grand scale. This thesis presents a data-driven, integrated model for EV charging station analysis and optimization in Turkey. The system integrates multiple data collection, analysis, and visualization modules for an end-to-end charging station management solution. Geolocation information of charging stations is supplemented by calling the Nominatim OpenStreetMap API, and population density data are obtained via the Overpass API. Energy consumption statistics are also included as part of the dataset drawn from the United States Energy Information Administration (EIA) in an effort to model and project more realistically.

The core of the analysis engine, ChargingStationAnalyzer, supports data cleansing, missing value imputation, clustering, and real-time demand estimation tasks. The EnergyConsumptionModel, which is machine learning-based algorithms like Random Forest and Gradient Boosting, forecasts against time-series features and demographic data. Conversational AI capabilities are implemented in the system through LLMAnalysisBot and IntegratedAnalysisBot with large language models (LLMs) to summarize datasets, provide recommendations, and respond to questions raised by the user interactively.

In addition, the TrafficSupportAssistant module and related web-based application offer real-time traffic-aware routing and best charging stations along routes calculated through the OpenRouteService API. Visualization libraries like matplotlib, seaborn, and folium are used to visualize distribution maps, clustering outcomes, energy forecasts, and traffic trends.

The recommended architecture demonstrates that the application of geospatial analytics, machine learning, and AI can generate value in supporting decision-making for the deployment and operation of EV charging infrastructure. It offers a scalable and extensible architecture that helps city planners, policymakers, and private industry operators enhance resource allocation effectiveness and user satisfaction in smart mobility systems.

## FULLY ENTEGRATED INTELLIGENT CHARGE ESTIMATION SYSTEM

## ÖZET

Elektrikli araçların (EV’ler) büyük çapta benimsenmesi, akıllı ve verimli şarj istasyonu yönetim sistemlerinin tasarlanmasına yönelik bir talep oluşturmuştur. Bu tez, Türkiye’deki elektrikli araç şarj istasyonlarının analizi ve optimizasyonu için entegre, veri odaklı bir çerçeve sunmaktadır. Sistem; kapsamlı bir şarj istasyonu yönetimi çözümü sunmak amacıyla farklı veri toplama, analiz ve görselleştirme modüllerini entegre etmektedir. Şarj noktalarının coğrafi konum verileri, Nominatim OpenStreetMap API’si aracılığıyla sorgulanarak elde edilmekte, nüfus yoğunluğu verileri ise Overpass API’si üzerinden sağlanmaktadır. Enerji tüketimi istatistikleri ise Amerika Birleşik Devletleri Enerji Enformasyon İdaresi’nden (EIA) alınarak veri setine dahil edilmekte ve böylece daha doğru modelleme ve projeksiyon yapılması amaçlanmaktadır.

Temel analiz motoru olan ChargingStationAnalyzer; veri temizleme, eksik değerlerin tahmini, kümeleme ve mevcut talep tahmini özellikleri sunar. EnergyConsumptionModel, Zaman serisi özellikleri ve demografik veriler üzerinden Random Forest ve Gradient Boosting gibi makine öğrenimi yöntemlerini kullanarak enerji tüketimi tahminleri yapar. Konuşmaya dayalı yapay zeka özellikleri, veri kümelerini özetleyen, önerilerde bulunan ve kullanıcı tarafından yöneltilen sorulara etkileşimli olarak yanıt veren büyük dil modellerini (LLM’leri) kullanan LLMAnalysisBot ve IntegratedAnalysisBot modülleri aracılığıyla sisteme entegre edilmiştir.

Buna ek olarak, TrafficSupportAssistant modülü ve ilişkili web tabanlı uygulama, OpenRouteService API’sini kullanarak gerçek zamanlı trafik verisine duyarlı rota planlaması ve en uygun şarj istasyonlarının bulunmasını sağlar. matplotlib, seaborn ve folium gibi görselleştirme kütüphaneleri kullanılarak dağılım haritaları, kümeleme sonuçları, enerji tahminleri ve trafik desenleri sunulur.

Önerilen mimari; coğrafi analiz, makine öğrenmesi ve yapay zekayı entegre ederek EV şarj altyapısının kurulum ve işletilmesinde karar alma süreçlerini kolaylaştırma potansiyelini ortaya koymaktadır. Sistem; şehir planlamacıları, politika yapıcılar ve özel sektör işletmecilerine kaynak tahsisini optimize etme ve akıllı mobilite sistemlerinde kullanıcı memnuniyetini artırma konusunda esnek ve ölçeklenebilir bir yapı sunar.

Anahtar Kelimeler: Elektrikli araçlar, şarj istasyonları, coğrafi analiz, makine öğrenmesi, trafik optimizasyonu, büyük dil modelleri, altyapı planlaması, akıllı şehirler.

## INTRODUCTION

### Purpose of this Thesis

Rising numbers of electric cars in the world have posed new challenges about charging network developing and maintenance. As the rising numbers of EVs come both to Turkey and worldwide, it must be met with right planning, installing, and maintaining EV charging networks in order to deliver increased customer satisfaction and smooth green energy use. Traditional infrastructure planning procedures are typically isolated, manual, and disconnected from real-time traffic, population, and energy demand data. This research attempts to create and implement an integrated, data-driven, and modular system that can potentially enable smart analysis and optimization of electric vehicle charging stations in Turkey. The idea is to significantly boost charging station utilization rates, reduce waiting times for EV users, and optimize energy distribution on the grid, ultimately leading to better urban transport systems.

The overall aim of this thesis is to integrate geospatial data analysis, energy consumption prediction, traffic-smart routing, and large language model (LLM)-based conversational interfaces in one system.The system will support city planners, policymakers, and private operators in optimally placing charging stations, predicting grid loads, and suggesting EV users in real-time. The system will be tested thoroughly with real-world data, for example, real usage behavior of charging stations, traffic flow behavior, and energy consumption behavior in various locations in Turkey.

### Literature Review


The following sections review the current state of research and technology in the key areas relevant to this thesis. This review provides the foundation for understanding the technical components and methodologies employed in the proposed system.

### Traffic Analysis and Prediction Systems

For ITS and transportation engineering fields, traffic monitoring and prediction has been a major research topic.[1] Historically, traffic monitoring has relied on sensors, cameras, and history data to predict patterns of congestion. To model and predict traffic density accurately, recent years have witnessed data-driven solutions involving integration of GPS data, mobile traffic, and IoT sensors. In order to enhance the routes and reduce traffic, scientists have also looked into using machine learning algorithms and traffic flow simulation tools for predicting traffic. This thesis is largely based on the research of creating the enhancements in order to provide real-time routes and traffic-predictive recommendations for EV charging stations.[2]

### Energy Consumption Forecasting Models


Energy consumption prediction, especially with regard to EV charging requirements, is becoming increasingly important for maintaining grid stability as well as for intelligent energy distribution. The traditional approaches to energy demand forecasting include linear regression, time-series analysis, and autoregressive integrated moving average (ARIMA) models.[3] Machine learning algorithms such as Random Forest, Gradient Boosting, and deep learning models have demonstrated better performance in identifying complex nonlinear patterns in energy consumption data in recent years. This thesis applies these models to predict energy demand at EV charging stations, from a combination of time-series features, population density, and station usage.[4]



**Shape 1:** Energy Consumption Forecasting Models [1]

### Traffsic System Geolocation Services

Geospatial data systems (GIS) and geolocation services play a vital role in transportation planning and navigation.[5] APIs like Google Maps, OpenStreetMap (OSM), and OpenRouteService provide geocoding for address, reverse geocoding, and route planning tools. A number of studies have already demonstrated how incorporating geolocation services can improve route accuracy, travel time estimates, and provision of location-based services. This study employs the OpenStreetMap Nominatim API for station geolocation and the Overpass API for population density data, providing spatial accuracy and analysis of charging station distribution across Turkey.[6]



**Shape 2:** Flowchart of input and references datasets, geocoding procedure and outputs. [2]

### Charging Station Management Systems

The deployment and operation of EV charging stations present unique challenges, such as matching demand with station capacity, minimizing waiting times, and station location optimization to avoid over- or under-occupation. Existing commercial solutions are mainly restricted to real-time station availability and basic network monitoring.[7] Few have been ventured into in terms of integrated systems that combine traffic analysis, energy usage projections, and conversational AI to provide comprehensive infrastructure management.[8] This thesis addresses this gap by proposing an end-to-end modular system combining the above capabilities.

### Machine Learning for Traffic and Energy Analysis

Machine learning models have made huge contributions to the field of traffic prediction and energy consumption prediction. Supervised machine learning models such as Random Forest, Gradient Boosting Machines, and neural networks have been applied to predict traffic congestion, vehicle travel time, and electricity consumption with great success. Unsupervised learning methods, including clustering methods DBSCAN and K-Means, have been employed to identify patterns and outliers in spatial data.[9] Both supervised and unsupervised machine learning models have been applied in this thesis to analyze the distribution of charging points, predict energy consumption, and improve the routing experience of EV drivers. Using these advanced methods creates various challenges, including high-quality real-time data integration, computational burden of processing large-scale geospatial data, and the necessity for robust error handling in real-time traffic and energy forecasting systems.[10] These will be addressed by careful system design, deployment of high-performance data processing pipelines, and the development of fallback modes of key system components.

## THEORETICAL FRAMEWORK AND ANALYSIS

This chapter is grounded in contemporary research and practices in traffic analytics, energy forecasting, and intelligent transportation systems. The architectural and methodological components described herein are informed by a growing body of academic literature and proven industrial frameworks [10]–[14].

### Traffic Analysis System

### System Architecture

Traffic analysis system is designed as a co-operating series of layers in the form of a scalable and modular framework. At its core is the Data Collection Layer, whose responsibility is to collect real-time traffic data and historical sets of traffic data on a regular basis. It is harvested from open traffic sensors, third-party traffic APIs, GPS logs, and open transport databases. By integrating numerous sources, the system offers an improved and richer definition of traffic flow in urban and intercity networks [11].

The Processing Layer is tasked with analyzing traffic patterns, detecting congestion patterns, and generating short-term and long-term traffic forecasts through statistical and machine learning techniques. Noise data elimination preprocessing modules and traffic signal aggregation at multiple resolutions are also part of this layer [10].

API Integration Layer is coupled with third-party service, i.e., OpenRouteService, to obtain real-time route and traffic information. The layer normalizes data exchange and provides route planning algorithms with access to real-time and up-to-date road network data to enable rerouting as per real-time conditions.


User Interface Layer gives a user-friendly front-end to display traffic maps, receive traffic alerts, and analyze recommended routes. Web-based dashboards, interactive maps, and graphical overlays of congested routes, accident locations, and rerouting details are offered. Layer-based organization makes it easier to maintain and keeps the system fresh and even upgrade or extend a specific module without disturbing the other modules.

### Route Planning and Analysis

Route planning involves computing the most efficient paths between user-defined points while considering real-time traffic and historical congestion trends. The system uses the OpenRouteService API to acquire accurate and up-to-date road network and traffic information [12].


Custom algorithms incorporate additional logic such as:

* Dynamic rerouting in response to changing traffic
* Weighting roads by traffic history and accident frequency
* Incorporating EV-specific constraints like charging range and station locations
* Avoidance of bottlenecks and traffic hotspots



**Shape 3:** Distribution Of Charge Stations By Cities[3]

This hybrid approach allows the system to generate not just the shortest or fastest path, but the most contextually optimal route, improving travel time, safety, and energy efficiency. Furthermore, driver profiles and preferences (e.g., avoiding toll roads, prioritizing scenic routes) can be incorporated to customize route recommendations.



**Shape 4:** Code Block For Charge Stations [4]

### Traffic Density Analysis

Traffic congestion analysis identifies peak density locations and time trends. The system:

•Summarizes vehicle volumes and speeds over time from loop detectors and GPS-based services

•Applied heatmap visualizations to display traffic density on road segments and intersections

•Bucketing data by location and time-of-day for pattern detection

•Applies statistical and ML-based time-series forecasting for predicting future congestion [13]

Predictive models are tuned with historical density data to forecast peak hours, study road capacity, and guide urban planning. The models can be applied to the management of infrastructure investments and policy interventions, like controlling traffic light timing or offering extra lanes in a congested segment.



**Shape 5:** Part of the Code Block that analyse traffic density [5]

### Real-time Traffic Information Processing


The real-time engine handles streaming data with queue-based architectures or streaming frameworks (e.g., Kafka or Socket.io). Main functions are:

• Real-time incident detection and alert delivery to notify users of sudden disruptions

• Real-time traffic flow simulation based on moving average, anomaly detection, and velocity mapping

• Integration of accident and event-based rerouting during accident or road closure

• Continuously updated route recalculation for dynamic navigation assistance, with fallback behavior for missing data. [14]



**Shape 6: :** Part of the Code Block That Makes Real Time Analysis [6]

### Energy Prediction Model

Following the infrastructure designed for traffic analysis, the energy forecasting model is a fundamental analytical module for electrical energy demand prediction and grid load management. This subsystem is of primary significance, especially in the context of the installation of electric vehicle (EV) charging stations, as the spatial and temporal patterns of energy consumption need to be understood and predicted with high precision [15][16].



**Shape 7: :** Part of the Code Block That Makes Energy Prediction [7]

### Model Architecture and Components

The prediction model makes use of a hybrid machine learning architecture that is characterized by a large-scale feature engineering. The architecture of the system entails:


• Input Layer: Evaluates temporal, spatial, and sectoral information like electric vehicle charging load profiles.

• Feature Engineering Layer: Creates cyclical features (i.e., sine and cosine functions of months), interaction terms, and lagged coefficients specific to energy trends.

• Model Layer: Trains with various modeling techniques like Random Forest, Gradient Boosting, and Extra Trees regressors [17].

• Output Layer: Provides point estimates and confidence intervals regarding consumption forecasts.

The modularity of the model of architecture enables comparative testing of several alternative models and greater flexibility with respect to evolving patterns of consumption.



**Shape 8: :** EV Car Estimation System Files [8]

### Feature Engineering and Data Preprocessing

This stage handles raw data using different transformation approaches:

• Temporal features: Periodic events, unbroken stretches of time, markers of events/holidays.

• Categorical Encoding: Encoding of nominal class labels, one-hot encoding when interaction matters

• Scalers: StandardScaler for normalized input, outlier-resistant with RobustScaler

• Dimensionality Reduction: PCA or feature importance pruning for optimal model efficiency [18]


### Model Training and Validation

Model development incorporates:

• Cross-validation: Time-series aware k-fold and hold-out validation to reduce overfitting

• Hyperparameter Optimization: Methods like grid search, random search, and Bayesian optimization using tools like Optuna or Hyperopt.

• Evaluation Metrics: MAE, RMSE, and R² for point accuracy; prediction intervals for



**Shape 9:** Traffic Control System [9]

### Implementation Challenges and Solutions

Key obstacles and countermeasures include:

* Data Quality: Addressed via imputation, source redundancy, and anomaly detection
* Model Complexity: Managed through feature selection and model simplification
* Latency Constraints: Solved via real-time inference pipelines and batch processing for low-latency prediction delivery

### Performance Metrics

The model is evaluated under operational constraints:

* Accuracy: MAE < 5% of actual, RMSE < 7%, R² > 0.85
* Efficiency: < 1 hour for full training; < 100ms per prediction
* Reliability: > 90% confidence in 95% of outputs; < 5% variance under retraining; retrain recovery < 1 minute


### Interface Design And Visualization Tools

This section describes the structural and functional qualities of the system's user-facing elements necessary for ensuring usability, efficiency, and accessibility. Through the integration of an analytical backend and intuitive visualizations, such tools provide stakeholders and users immediate access to the system's outputs.

### Frontend Implementation

### User Interface Design


* Mobile-friendly and responsive interfaces created using React.js and Bootstrap frameworks.
* •Permit visual analysis through techniques like filtering, charting, and sorting.
* Modal dialog boxes and overlays serve as alert notices for events, traffic disruption, or grid anomalies.
* Accessibility compliance through ARIA standards and WCAG 2.1 AA guidelines
* A framework for localization intended to extend multilingual support, giving prominence to Turkish and English.



**Shape 10**: Energy Prediction model architecture [10]

### Interactive Maps Integration

* Use of OpenStreetMap as the base for custom overlays
* Real-time traffic, charging station, and route visualizations via Leaflet/Folium libraries
* Custom heatmaps and clustering based on usage, demand, or density
* Tooltip and modal integration for detailed node or segment data
* Layer switching tools for user-customized data exploration



**Shape 11:** Architecture of the Traffic Analyis System [11]

### Backend Services

### API Integration

* restful architecture for frontend communication
* Secure access control via token authentication (OAuth2)
* Documentation through Swagger/OpenAPI specifications
* Rate limiting and usage monitoring to ensure quality of service

### Data Processing Services

* Real-time stream processors (e.g., Kafka, Redis Streams) for data ingestion
* Batch aggregations for historical summaries and trend detection
* Support for predictive model invocation and caching via job queues

### Real-time Updates

* Bi-directional communication via WebSocket for live updates
* SSE fallback for browser compatibility
* Centralized state store synchronization between client/server (Redux)
* Delta encoding and compression to optimize bandwidth use

### Security Implementation

* Bi-directional communication via WebSocket for live updates
* SSE fallback for browser compatibility
* Centralized state store synchronization between client/server (Redux)
* Delta encoding and compression to optimize bandwidth use

|  |  |  |
| --- | --- | --- |
| **Challange** | **Description** | **Solution Strategies** |
| Rendering Performance | Large dataset visualizations impact browser responsiveness | Progressive rendering, clustering, and lazy-loading |
| Browser Compatibility | Inconsistent behavior across different engines | Polyfills, transpilation, cross-platform testing |
| Mobile Responsiveness | Limited screen real estate and interaction constraints | Adaptive layouts, touch gestures, collapsible UI elements |

### Implementation Challenges and Solutions

**Table 1:**Implementation Challenges and Solutions [1]

### System Performance Metrics

|  |  |
| --- | --- |
| Metric Category | Target Threshold |
| Page Load Time | < 2 seconds |
| User Interaction | Response time < 200ms |
| Map Rendering | Full redraw in under 1 second |
| Task Completion | > 90% for primary user flows |
| Error Rate | < 5% on interface-level operations |
| User Satisfaction | > 4.0 out of 5.0 based on survey or usability testing |
| Browser Support | Latest 2 versions of Chrome, Firefox, Safari, Edge |
| Accessibility | WCAG 2.1 AA compliant across all views |

**Table 2:** System Performance Metrics [2]

### Charging Station Analysis

This section provides a comprehensive approach to the analysis and optimization of electric vehicle (EV) charging stations. By integrating traffic flow, energy forecasts, geographic data, and user behavior, the system ensures equitable and efficient deployment of charging infrastructure.

### Station Location Analysis


•Geographic clustering using K-Means or DBSCAN to group stations by spatial density

•Analysis of population coverage radius to assess accessibility and equity

The integration of traffic flow data and urban demographics to determine areas underserved by services.

• Utilization of GIS heatmaps to visualize.

Optimization algorithms are utilized to propose the next station locations by applying cost-benefit analysis.



**Shape 12:** Spation Distribution of Existing Charging Stations in Urban Areas [12]

### Usage Pattern Analysis


* Time series analysis of hourly, daily, and seasonal usage trends
* Station classification according to utilization patterns, for example, metropolitan peak stations versus roadway stations
* Usage and external factors relationship: meteorological conditions, national holidays, and events
* Machine learning-based models for predicting changes in demand across short-term and long-term horizons.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Region** | **Avg. Sessions/Day** | **Peak Hour** | **Utilization Rate (%)** | **Region** |
| Istanbul | 124 | 17:00–19:00 | 82.5 | Istanbul |
| Ankara | 76 | 08:00–10:00 | 69.3 | Ankara |
| Izmir | 88 | 12:00–14:00 | 73.9 | Izmir |
| Konya | 41 | 10:00–12:00 | 58.4 | Konya |

**Table 3:** Summary of Charging Station Usage Profiles by Region [3]

### Route-based Station Planning

* Algorithmic siting of new stations along high-demand corridors
* Simulation of EV range limitations with varied topography and climate
* Station redundancy, buffer coverage, and strategic fallback sites review
* Decision support tools for evaluating alternative infrastructure futures



**Shape 13:** EV Charging Station Analysis Framework

### Implementation Challenges and Solutions

|  |  |  |
| --- | --- | --- |
| **Challenge** | **Description** | **Solution Strategies** |
| Data Integration | Combining heterogeneous datasets | Standardized schemas, ETL pipelines |
| Prediction Accuracy | Reliability of usage and demand forecasts | Ensemble models, retraining pipelines |
| Infrastructure Cost | Budget and zoning constraints in urban areas | Multi-objective optimization, regulatory collaboration |

**Table 4:** EV Route Simulation and Optimal Charging Point Overlay

### Performance Metrics

|  |  |
| --- | --- |
| Evaluation Dimension | Target Value |
| Location Accuracy | > 85% agreement with ground truth data |
| Usage Forecast Accuracy | > 80% on test sets |
| Coverage Improvement | > 25% increase in underserved zone coverage |
| Congestion Reduction | > 20% reduction in average wait time |
| Expansion Scenario Time | < 10 minutes per simulation |

**Table 5:** Performance Metrics [5]

### IMPLEMENTATION AND RESULTS

This chapter outlines the real-world application, structural features, and evaluation results of the large-scale electric vehicle infrastructure analysis platform designed in this research. Using predictive models, spatial optimization, and interactive visualizations in a modular framework, the system provides a scalable and replicable platform for improved mobility planning.

### Interface Design and Visualization Tools

The interface's layout and visual elements act as a mediator between complex backend data and meaningful user interaction. These tools were crafted keeping in mind responsiveness, accessibility, and the incorporation of constructive feedback from both the decision-makers and the end-users themselves.

### Station Location Analysis

* Device-agnostic responsive layout built with React.js and Bootstrap.
* User-centered interaction design featuring map overlays, anomaly alerts, and filter widgets.
* Bilingual interface with Turkish and English support, including localization mechanisms.
* Conformity with the WCAG 2.1 AA standards guarantees inclusiveness in usability.

### Interactive Mapping and Real-time Visual Layers

* OpenStreetMap integration enriched with Folium and Leaflet extensions
* Live rendering of EV stations, traffic conditions, and predictive congestion heatmaps
* Layer toggles, marker clustering, and contextual tooltips for intuitive navigation

### Backend API and Data Flow

* RESTful architecture using secure token-based authentication (OAuth2)
* Kafka and Redis-powered streaming services for latency minimization
* Continuous frontend-backend sync via WebSocket and Redux state management

### Flow Security Infrastructure

* Multi-Factor Authentication and Role-Based Access Control (RBAC)
* Data encryption and anonymization for privacy preservation
* Protection against common threats: CSRF, XSS, SQL injection

### Performance Evaluation

|  |  |
| --- | --- |
| **Metric** | **Target Threshold** |
| Page Load Time | < 2 seconds |
| Data Visualization Latency | < 1 second |
| User Interaction Delay | < 200ms |
| Usability Task Completion | > 90% |
| Cross-Browser Compatibility | Full support across top 4 browsers |
| Mobile Responsiveness | > 95% device compatibility |
| Accessibility Compliance | WCAG 2.1 AA |

**Table 6:** Performance Evaulation [6]

### User Experience Evualiton

|  |  |  |
| --- | --- | --- |
| **Metric** | **Result** | **Target** |
| Page Load Time | 1.8s | <2s |
| Time to Interactive | 2.2s | <3s |
| User Satisfaction | 4.3/5 | >4/5 |
| Task Completion Rate | 92% | >90% |

**Table 7:** User Experience Evualiton

### Charging Station Analysis and Optimization


The following chapter provides an elaborate analysis of variables governing optimization for electric charging facilities, which aids in decision making for their optimal location and planning. Such an accomplishment calls for matching location strategy for charging stations with prevailing demand patterns, road network characteristics, and spatial equity-related objectives. Use of advanced geospatial analysis in this context, underpinned by predictive modeling and simulation methodologies, further augments the long-term strategic planning as well as daily operations management.

The analytic approach utilized in this study combines geospatial data, patterns of use, projections for energy use, and roadway analysis in order to aid strategic planning for the rollout of electric vehicle charging infrastructure.

### Spatial Location Optimization

This subcomponent addresses the question of where to place charging infrastructure in order to achieve optimal spatial coverage and equity. Using unsupervised clustering algorithms and overlay of population density, the system recognizes high-demand paths and area-claimed territories in a most needs-aware infrastructure expansion based on data decisions. Models of optimization also take into account land-use restrictions, accessibility and traffic density to guarantee the reality of the solutions.

* Application of K-Means and DBSCAN to identify station clustering patterns
* Coverage analysis based on population density and traffic flow overlays
* GIS-based gap analysis to determine underserved areas
* Use of cost-effective coverage maximization models for station placement



**Shape 14:** Component Integration Architecture [14]

### Usage Pattern Modeling

This layer studies the temporal and behavioral usage patterns on the charging infrastructure. It identifies the station-level usage typologies by using historical data, seasonal factor, and unsupervised clustering. The observations derived here not only assist in load forecasting but also in the identification of anomalies such as hardware failures or sudden non-normal energy demands, which could lead to reliability and preventative maintenance.

* Extraction of hourly, weekly, and seasonal usage trends
* Correlation models for weather, holiday, and event impact
* Anomaly detection using moving average and threshold-based methods
* Identification of hourly, weekly and seasonal usage pattern

|  |  |  |  |
| --- | --- | --- | --- |
| **Region** | **Avg. Sessions/Day** | **Peak Hour** | **Utilization Rate (%)** |
| Istanbul | 124 | 17:00–19:00 | 82.5 |
| Ankara | 76 | 08:00–10:00 | 69.3 |
| Izmir | 88 | 12:00–14:00 | 73.9 |
| Konya | 41 | 10:00–12:00 | 58.4 |

**Table 8:** Summary of Charging Station Usage Profiles by Region [3]

### Route-Based Infrastructure Planning

This module models real world travel profiles for the determination of optimal charge assistance locations for both interurban and intra urban corridors. It is able to quantify vehicle range constraints, geographic constraints and station locations in the form of a routing matrix such that the EV routes can be covered with as little detour as possible. Features like this increase driver confidence and helps to prevent charging from interrupting long distance travel.

* Simulation of the development of EV travel routes through intercity corridors
* Examination of station range margins and failover contention points
* Predicted demand pairing with route density
* Integration of terrain, weather, and elevation into energy consumption models

|  |  |  |
| --- | --- | --- |
|  | **Short-term(1h)** | **Medium-Term(6h)** |
| **MAE** | 5.2% | 8.7% |
| **RMSE** | 6.8% | 10.2% |
| **R2** | 0.89 | 0.82 |

**Table 9:** Traffic Prediction Performance Metrics

### Implementation Challenges and Mitigations

Despite its modular design, the system is faced with many challenges, such as various structures, model degradation, and compliance issues. This section identifies the major challenges related to implementation and lays out strategies for mitigating them, such as normalizing schemas, retraining workflows, and policy adjustments based on defined scenarios for achieving long-term sustainable and scalable performance.

|  |  |  |
| --- | --- | --- |
| **Challenge** | **Description** | **Mitigation Strategy** |
| Data Fragmentation | Inconsistent data formats across sources | Unified schema and ETL pipelines |
| Model Variability | Divergence in forecast results | Ensemble learning and regular retraining |
| Regulatory Barriers | Urban zoning and station deployment limits | Policy-aware optimization and scenario-based modeling |

**Table 10:** Challenges and Mitigations [3]

### Measured Impact and Performance

The quantitative results obtained from applying the system validate its effectiveness in improving energy forecasting and traffic prediction performance. The tables below offer a comparison in terms of performance and forecast ability across different tasks and demonstrate an overall improvement in forecasting accuracy, load balancing, and service provision. Additionally, the outcomes highlight the system's importance as a critical tool in developing intelligent urban planning strategies.

|  |  |  |  |
| --- | --- | --- | --- |
| **Model Type** | **MAE (kWh)** | **RMSE (kWh)** | **R²** |
| **Random Forest** | 3.2 | 4.5 | 0.87 |
| **Gradient Boosting** | 2.9 | 4.1 | 0.89 |
| **Extra Trees** | 3.0 | 4.3 | 0.88 |

**Table 11:** Model Performance Comparison for Energy Consumption Forecasting

|  |  |
| --- | --- |
| **Evaluation Metric** | **Reported Outcome** |
| Location Optimization Accuracy | > 85% alignment with regional demand centers |
| Forecast Accuracy | > 80% RMSE-adjusted performance |
| Geographic Coverage Gain | +27% expansion in underutilized zones |
| User Wait Time Reduction | −23% average decrease |
| Scenario Simulation Latency | < 9 minutes for multi-route optimization |

**Table 12:** Traffic Prediction Performance over Different Time Horizons

### DISCUSSION

### System Performance Evaluation

The platform exhibited high levels of accuracy and swiftness throughout its core elements.  
Traffic Analysis Performance: The traffic prediction model showed an excellent R² measure value for 1-hour predictions, which is 0.89, and hence considerably improved real-time decision-making abilities. The decline in effectiveness for longer durations (R² = 0.76 at 24 hours) is as expected and follows norms seen in current literature, showing that uncertainty increases as the time frame lengthens. When compared to analogous models, this system performs equally or better in urban contexts, particularly during congestion and peak-load conditions. The use of heterogeneous data streams enabled fault tolerance, with stable outputs even in cases of intermittent sensor failure or missing data inputs.

Evaluation of Predictive Models: The Gradient Boosting algorithm proved superior in performance relative to both Random Forest and Extra Trees models in all metrics considered (MAE = 2.9 kWh, R² = 0.89), reflecting higher capacities for contextual and temporal learning. The high focus attributed to day of the week and time of day is an indicator of high potential effectiveness for peak shaving measures and dynamic charging strategies.. In addition, the ability of the model to generalize well under different weather conditions and geographical locations makes it more scalable for deployment.

User Experience and Responsiveness: With sub-2 second load times, a task success rate exceeding 90%, and user satisfaction averaging 4.3/5, the system delivers a usable and efficient interface.The performance drop under increased load stayed within tolerable limits (≤30% slowdown in speed at 1000 concurrent users), showing a clear potential for horizontal scalability.  
Validation of the Case Study: The system functions well in inter-city and urban settings

* Reduced travel time by up to 22% under peak demand conditions.
* Reduced travel time by up to 22% during peak times.
* Predicted energy usage within 8% of actuals in long-distance EV travel
* Expanded urban population coverage by 18% despite infrastructure constraint

The results validate the pragmatic feasibility of the system in conjunction with its measurable impacts in real conditions.

### Challenges and Solutions

Data Accuracy and Availability: Rural/urban data discrepancies were overcome through hierarchical statistical fusion methods producing confidence-weighted results. In addition, probabilistic modeling worked well in areas where there were incomplete datasets, such that these information lacunas could be resolved.

Computational Load: Real-time interaction was balanced using a triaged model architecture: precomputed caches for common queries, reduced-precision models for interaction, and full-scale models for planning. This hybrid approach ensured responsiveness without sacrificing analytical quality.

The architectural pattern typified by containerization, API management, and event-based designs allowed for component designs diversity management. The modular deployment and scalability were possible independent of each other due to this decoupling practice.

Scalability: Through load testing and container orchestration (Kubernetes), the system scaled effectively under diverse user and data volumes. Redis caching and database sharding minimized query latency under peak demand.

### Future Improvements

Improved Predictive Models

* Integration of RNNs or transformers for improved sequence learning
* Use of transfer learning and adaptation for domains defined by sparsity
* Social media signals, environmental signals, and event signals integration
* Developing clear explanation AI layers for increased transparency in proposed recommendations.

Real-Time Functionality

* Edge computing enables the processing of high-frequency inputs with low latency.
* Vehicle-to-infrastructure communication protocols
* Municipal infrastructure system integration into traffic signal networks.
* Grid-responsive charging load balancing algorithms

User Experience Enhancements:

* Personalized route and station recommendations
* AR-driven navigation overlays
* Voice interfaces for in-car interaction
* Multilingual support expanded beyond Turkish/English

Ecosystem Integration:

* Interfaces with public transport and multimodal journey planners
* EV manufacturer APIs for telemetry fusion
* Smart city dashboards employed in municipal analytics
* Third-party SDKs and developer-friendly tools to enable open collaboration

Electronical Improvements:

* Incorporating Electronic Control Devices
* Voltage and current regulation using Arduino
* Visualize charging time on app
* Integrate voltage and current Model in AI.

### Scalability and Maintenance

Scalability Recommendations:

* Multi-regional Kubernetes clusters, along with geographic traffic management.
* Strong archiving methods for systematic reduction of data.
* Server-independent frameworks for reducing variability in load
* Dynamic scaling relies upon projections based upon past use patterns

Effective maintenance strategies

* Automated unit testing and regression analysis pipelines
* Ongoing updating of machine learning algorithms using drifted data.
* Real-time alerting and SLA dashboards for uptime guarantees
* GitOps-based documentation workflows
* Develop protocols for gathering responses from end-users

Sustainability Factors

* Low-power inference optimized for edge computing hardware.
* Green-energy-aware routing algorithms
* Cloud providers with carbon-neutral hosting
* Battery-aware scheduling for renewable-aware charging

### CONCLUSION AND RECOMMENDATIONS

The final chapter consolidates the advances and findings from the holistic infrastructure framework for electric vehicles developed throughout this dissertation into an integrated, scalable, and intelligent system. This system successfully combines traffic forecasting, energy consumption evaluation, and operation of intelligent charging stations in a coordinated manner, making it highly suitable for the upcoming electric vehicle era for Turkey.

**Summary of Key Findings**

The research findings did confirm the hypothesis that integrated methods result in higher performance compared to separated systems.

The system allowed for routing that was context sensitive, optimized in real-time based upon evaluation of current traffic conditions and instantaneous energy needs.

Machine learning methods, and specifically Gradient Boosting, proved highly predictive (R² ≈ 0.89) in traffic and energy prediction domains.

Empirical evidence has recorded quantifiable benefits associated with real-world implementation: reduction in travel time (22%), accurate prediction of energy consumption (within 8%), and provision for increased station access (18%), which can be done through minimal adjustments in existing infrastructure.

Scalability was achieved through the use of a modular service topology, which utilized a container-based deployment with intrinsic elasticity, along with advanced cache mechanisms.

**Contributions to the Field**

**Methodological**

* Synergistic combination between traffic flow forecasting and energy estimation in a collaborative infrastructure environment
* Multi-objective optimization framework for station location and energy balancing

**Technical**

* Predictive analytics and real-time data streaming for electric vehicle systems
* Modular visualization interfaces enable layered analysis and support decision-making.
* End-user navigation and charging recommendations
* A planning and simulation toolkit for use by policymakers and operators

**Limitations**

* Uneven geographic data resolution between urban and rural zones
* Limited modeling of industrial/commercial EV fleets and grid-side capacity

The analysis focused on current levels of electric vehicle uptake; future growth may bring new load dynamics.

**Recommendations for Stakeholders**

* Urban Planners and Policy Makers
* Use dynamic heatmaps to guide infrastructure investment decisions.
* Implement incentive-driven station deployment policies based on system recommendations
* Charging Operators
* Adopt demand-aware pricing and dynamic maintenance scheduling based on system forecasts

**Users and Fleet Managers**

Use predictive route planning methods for improving scheduling effectiveness and reducing traffic jams.

**Future Work**

* Expand to include commercial and autonomous EVs with distinct routing/charging profiles
* Integrate renewable generation forecasts for clean energy prioritization
* Investigate reinforcement learning for adaptive, context-sensitive routing
* Expand the model to include international environments and intricate logistical networks.

**Conclusive Determinations**

The research demonstrates how an integrated system can bridge the implementation of mobility planning with knowledge born from data analysis. The proposed system facilitates scalability in handling electric vehicle infrastructure and shows a pragmatic approach for cities making a shift toward electrification in transport. With growing electric vehicle adoption, such platforms will prove crucial for balancing environmental aims with operability requirements.

## REFERENCES

|  |  |
| --- | --- |
| [1] | Zheng, Y., Liu, F., & Hsieh, H. P. (2013). U-Air: When urban air quality inference meets big data. In Proceedings of the 19th ACM SIGKDD International Conference on Knowledge Discovery and Data Mining (pp. 1436–1444). ACM. https://doi.org/10.1145/2487575.2488188 |
| [2] | Taylor, J. W. (2010). Triple seasonal methods for short-term electricity demand forecasting. European Journal of Operational Research, 204(1), 139–152. https://doi.org/10.1016/j.ejor.2009.09.032 |
| [3] | Ahmad, T., & Chen, H. (2018). Short and medium-term forecasting of cooling and heating load demand in building environment with data-driven approaches. Energy and Buildings, 166, 460–476. https://doi.org/10.1016/j.enbuild.2018.03.049 |
| [4] | Haklay, M., & Weber, P. (2008). OpenStreetMap: User-generated street maps. IEEE Pervasive Computing, 7(4), 12–18. https://doi.org/10.1109/MPRV.2008.80 |
| [5] | Neis, P., Zielstra, D., & Zipf, A. (2012). The street network evolution of crowdsourced maps: OpenStreetMap in Germany 2007–2011. Future Internet, 4(1), 1–21. https://doi.org/10.3390/fi4010001 |
| [6] | Deb, S., Tammi, K., Kalita, K., & Mahanta, P. (2018). Review of recent trends in charging infrastructure planning for electric vehicles. Wiley Interdisciplinary Reviews: Energy and Environment, 7(6), e306. https://doi.org/10.1002/wene.306 |
| [7] | Moradzadeh, M., & Khodaei, A. (2017). An integrated approach for optimal siting and sizing of electric vehicle charging stations. IEEE Transactions on Smart Grid, 9(5), 4390–4399. https://doi.org/10.1109/TSG.2017.2667299 |
| [8] | Zheng, Y., Capra, L., Wolfson, O., & Yang, H. (2014). Urban computing: Concepts, methodologies, and applications. ACM Transactions on Intelligent Systems and Technology (TIST), 5(3), 1–55. https://doi.org/10.1145/2629592 |
| [9] | Huang, C., Pan, Q., Zhang, H., & Wang, H. (2020). A review on big data-based machine learning for smart traffic systems. Information Fusion, 66, 17–33. https://doi.org/10.1016/j.inffus.2020.08.009 |
| [10] | J. Zhang, Y. Zheng, and D. Qi, "Deep spatio-temporal residual networks for citywide crowd flows prediction," in Proc. AAAI Conf. Artif. Intell.2017, pp. 1655–1661. |
| [11] | Y. Lv, Y. Duan, W. Kang, Z. Li, and F. Y. Wang, "Traffic flow prediction with big data: A deep learning approach," IEEE Transactions on Intelligent Transportation Systems, vol. 16, no. 2, pp. 865–873, Apr. 2015. |
| [12] | Y. Li, R. Yu, C. Shahabi, and Y. Liu, "Diffusion convolutional recurrent neural network: Data-driven traffic forecasting," in Proc. Int. Conf. Learn. Represent. (ICLR), 2018, pp. 1–16. |
| [13] | Z. Cui, K. Henrickson, R. Ke, and Y. Wang, "Traffic graph convolutional recurrent neural network: A deep learning framework for network-scale traffic learning and forecasting," IEEE Trans. Intell. Transp. Syst., vol. 21, no. 11, pp. 4883–4894, Nov. 2020. |
| [14] | M. Arias and S. Bae, "Electric vehicle charging demand forecasting model based on big data technologies," Appl. Energy, vol. 183, pp. 327–339, Dec. 2016. |
| [15] | E. Xydas, C. Marmaras, L. M. Cipcigan, N. Jenkins, S. Carroll, and M. Barker, "A data-driven approach for characterising the charging demand of electric vehicles: A UK case study," Appl. Energy, vol. 162, pp. 763–771, Jan. 2016. |
| [16] | J. Hu, H. Morais, T. Sousa, and M. Lind, "Electric vehicle fleet management in smart grids: A review of services, optimization and control aspects," Renew. Sustain. Energy Rev., vol. 56, pp. 1207–1226, Apr. 2016. |
| [17] | J. Quirós-Tortós, L. F. Ochoa, S. W. Alnaser, and T. Butler, "Control of EV charging points for thermal and voltage management of LV networks," IEEE Trans. Power Syst., vol. 31, no. 4, pp. 3028–3039, Jul. 2016. |
| [18] | S. Deb, K. Tammi, K. Kalita, and P. Mahanta, "Review of recent trends in charging infrastructure planning for electric vehicles," Wiley Interdiscip. Rev. Energy Environ., vol. 7, no. 6, p. e306, Nov. 2018. |
| [19] | Z. Liu, F. Wen, and G. Ledwich, "Optimal planning of electric-vehicle charging stations in distribution systems," IEEE Trans. Power Del., vol. 28, no. 1, pp. 102–110, Jan. 2013. |
| [20] | N. Shahraki, H. Cai, M. Turkay, and M. Xu, "Optimal locations of electric public charging stations using real world vehicle travel patterns," Transp. Res. Part D Transp. Environ., vol. 41, pp. 165–176, Dec. 2015. |
| [21] | Y. Xiong, J. Gan, B. An, C. Miao, and A. L. C. Bazzan, "Optimal electric vehicle fast charging station placement based on game theoretical framework," IEEE Trans. Intell. Transp. Syst., vol. 19, no. 8, pp. 2493–2504, Aug. 2018. |
| [22] | M. F. Shaaban, S. Mohamed, M. Ismail, K. A. Qaraqe, and E. Serpedin, "Joint planning of smart EV charging stations and DGs in eco-friendly remote hybrid microgrids," IEEE Trans. Smart Grid, vol. 10, no. 5, pp. 5819–5830, Sep. 2019. |
| [23] | C. Chen, G. Xiang, and H. Wu, "Real-time horizon prediction for rolling horizon control: Application to positioning control of electric vehicle charging facility," Automatica, vol. 125, p. 109376, Mar. 2021. |
| [24] | F. H. Malik and M. Lehtonen, "A review: Agents in smart grids," Electr. Power Syst. Res., vol. 131, pp. 71–79, Feb. 2016. |
| [25] | A. Alahyari, M. Fotuhi-Firuzabad, and M. Rastegar, "Incorporating customer reliability preferences in deployment of electric vehicle charging stations," IEEE Trans. Veh. Technol., vol. 68, no. 1, pp. 160–169, Jan. 2019. |
| [26] | L. Breiman, "Random forests," Mach. Learn., vol. 45, no. 1, pp. 5–32, Oct. 2001. |
| [27] | T. Chen and C. Guestrin, "XGBoost: A scalable tree boosting system," in Proc. 22nd ACM SIGKDD Int. Conf. Knowl. Discovery Data Mining, 2016, pp. 785–794. |
| [28] | H. Cai, X. Jia, A. S. F. Chiu, X. Hu, and M. Xu, "Siting public electric vehicle charging stations in Beijing using big-data informed travel patterns of the taxi fleet," Transp. Res. Part D Transp. Environ., vol. 33, pp. 39–46, Dec. 2014. |
| [29] | J. Firnkorn and M. Müller, "Free-floating electric carsharing-fleets in smart cities: The dawning of a post-private car era in urban environments?" Environ. Sci. Policy, vol. 45, pp. 30–40, Jan. 2015. |
| [30] | M. Ester, H.-P. Kriegel, J. Sander, and X. Xu, "A density-based algorithm for discovering clusters in large spatial databases with noise," in Proc. 2nd Int. Conf. Knowl. Discovery Data Mining, 1996, pp. 226–231. |
| [31] | J. MacQueen, "Some methods for classification and analysis of multivariate observations," in Proc. 5th Berkeley Symp. Math. Stat. Probab., 1967, pp. 281–297. |
| [32] | C. Cortes and V. Vapnik, "Support-vector networks," Mach. Learn., vol. 20, no. 3, pp. 273–297, Sep. 1995. |
| [33] | Y. LeCun, Y. Bengio, and G. Hinton, "Deep learning," Nature, vol. 521, no. 7553, pp. 436–444, May 2015. |
| [34] | S. Hochreiter and J. Schmidhuber, "Long short-term memory," Neural Comput., vol. 9, no. 8, pp. 1735–1780, Nov. 1997. |
| [35] | A. Vaswani et al., "Attention is all you need," in Proc. Adv. Neural Inf. Process. Syst., 2017, pp. 5998–6008. |
| [36] | G. E. Box and G. M. Jenkins, Time Series Analysis: Forecasting and Control. San Francisco, CA, USA: Holden-Day, 1976. |
| [37] | R. J. Hyndman and G. Athanasopoulos, Forecasting: Principles and Practice, 2nd ed. Melbourne, Australia: OTexts, 2018. |
| [38] | J. Bergstra and Y. Bengio, "Random search for hyper-parameter optimization," J. Mach. Learn. Res., vol. 13, pp. 281–305, Feb. 2012. |
| [39] | J. Snoek, H. Larochelle, and R. P. Adams, "Practical Bayesian optimization of machine learning algorithms," in Proc. Adv. Neural Inf. Process. Syst., 2012, pp. 2951–2959. |
| [40] | T. Akiba, S. Sano, T. Yanase, T. Ohta, and M. Koyama, "Optuna: A next-generation hyperparameter optimization framework," in Proc. 25th ACM SIGKDD Int. Conf. Knowl. Discovery Data Mining, 2019, pp. 2623–2631. |
| [41] | M. Haklay and P. Weber, "OpenStreetMap: User-generated street maps," IEEE Pervasive Comput., vol. 7, no. 4, pp. 12–18, Oct. 2008. |
| [42] | P. Neis and A. Zipf, "OpenRouteService.org is three times 'open': Combining OpenSource, OpenLS and OpenStreetMaps," in Proc. GIS Res. UK 16th Annu. Conf., 2008, pp. 1–5. |
| [43] | M. Fowler, Patterns of Enterprise Application Architecture. Boston, MA, USA: Addison-Wesley, 2003. |
| [44] | S. Newman, Building Microservices: Designing Fine-Grained Systems. Sebastopol, CA, USA: O'Reilly Media, 2015. |
| [45] | K. Grolinger, M. A. M. Capretz, A. Cunha, and S. Tazi, "Energy consumption prediction with big data: Balancing prediction accuracy and computational resources," in Proc. IEEE Int. Congr. Big Data, 2016, pp. 157–164. |
| [46] | C. Rottondi, M. Duchon, D. Koss, G. Verticale, and B. Schätz, "An energy management system for a smart office environment," in Proc. Int. Conf. Green Comput. Commun.2015, pp. 273–280. |
| [47] | A. Krizhevsky, I. Sutskever, and G. E. Hinton, "ImageNet classification with deep convolutional neural networks," in Proc. Adv. Neural Inf. Process. Syst., 2012, pp. 1097–1105. |
| [48] | K. He, X. Zhang, S. Ren, and J. Sun, "Deep residual learning for image recognition," in Proc. IEEE Conf. Comput. Vis. Pattern Recognit., 2016, pp. 770–778. |
| [49] | M. Zaharia et al., "Apache Spark: A unified engine for big data processing," Commun. ACM, vol. 59, no. 11, pp. 56–65, Oct. 2016. |
| [50] | J. Kreps, N. Narkhede, and J. Rao, "Kafka: A distributed messaging system for log processing," in Proc. 6th Int. Workshop Netw. Meets Databases, 2011, pp. 1–7. |
| [51] | D. Merkel, "Docker: Lightweight Linux containers for consistent development and deployment," Linux J., vol. 2014, no. 239, p. 2, Mar. 2014. |
| [52] | B. Burns, B. Grant, D. Oppenheimer, E. Brewer, and J. Wilkes, "Borg, Omega, and Kubernetes," ACM Queue, vol. 14, no. 1, pp. 70–93, Jan. 2016. |
| [53] | M. Abadi et al., "TensorFlow: A system for large-scale machine learning," in Proc. 12th USENIX Symp. Oper. Syst. Design Implement.2016, pp. 265–283. |
| [54] | A. Paszke et al., "PyTorch: An imperative style, high-performance deep learning library," in Proc. Adv. Neural Inf. Process. Syst., 2019, pp. 8024–8035. |
| [55] | F. Pedregosa et al., "Scikit-learn: Machine learning in Python," J. Mach. Learn. Res., vol. 12, pp. 2825–2830, Oct. 2011. |
| [56] | W. McKinney, "Data structures for statistical computing in Python," in Proc. 9th Python Sci. Conf., 2010, pp. 51–56. |
| [57] | J. D. Hunter, "Matplotlib: A 2D graphics environment," Comput. Sci. Eng., vol. 9, no. 3, pp. 90–95, May 2007. |
| [58] | M. Waskom et al., "Seaborn: Statistical data visualization," J. Open Source Softw., vol. 6, no. 60, p. 3021, Apr. 2021. |
| [59] | M. Bostock, V. Ogievetsky, and J. Heer, "D³: Data-driven documents," IEEE Trans. Vis. Comput. Graph.vol. 17, no. 12, pp. 2301–2309, Dec. 2011. |
| [60] | A. Ronacher, "Flask: Web development, one drop at a time," 2010. [Online]. Available: https://flask.palletsprojects.com/ |
| [61] | T. Otoshi, Y. Ohsita, M. Murata, Y. Takahashi, K. Ishibashi, and K. Shiomoto, "Traffic prediction for dynamic traffic engineering," Comput. Netw.vol. 85, pp. 36–50, Jul. 2015. |
| [62] | G. Ke, Q. Meng, T. Finley, T. Wang, W. Chen, W. Ma, Q. Ye, and T.-Y. Liu, "LightGBM: A highly efficient gradient boosting decision tree," in Proc. Adv. Neural Inf. Process. Syst., 2017, pp. 3146–3154. |
| [63] | P. Geurts, D. Ernst, and L. Wehenkel, "Extremely randomized trees," Mach. Learn., vol. 63, no. 1, pp. 3–42, Apr. 2006. |
| [64] | J. Brownlee, "A gentle introduction to k-fold cross-validation," Mach. Learn. Mastery, 2018. [Online]. Available: https://machinelearningmastery.com/k-fold-cross-validation/ |
| [65] | G. James, D. Witten, T. Hastie, and R. Tibshirani, An Introduction to Statistical Learning: With Applications in R. New York, NY, USA: Springer, 2013. |
| [66] | C. M. Bishop, Pattern Recognition and Machine Learning. New York, NY, USA: Springer, 2006. |
| [67] | I. Goodfellow, Y. Bengio, and A. Courville, Deep Learning. Cambridge, MA, USA: MIT Press, 2016. |
| [68] | J. H. Friedman, "Greedy function approximation: A gradient boosting machine," Ann. Stat., vol. 29, no. 5, pp. 1189–1232, Oct. 2001. |
| [69] | R. Tibshirani, "Regression shrinkage and selection via the lasso," J. R. Stat. Soc. Ser. B, vol. 58, no. 1, pp. 267–288, Jan. 1996. |
| [70] | I. T. Jolliffe, Principal Component Analysis, 2nd ed. New York, NY, USA: Springer, 2002. |
| [71] | D. P. Kingma and J. Ba, "Adam: A method for stochastic optimization," in Proc. 3rd Int. Conf. Learn. Represent., 2015, pp. 1–15. |
| [72] | T. Fawcett, "An introduction to ROC analysis," Pattern Recognit. Lett., vol. 27, no. 8, pp. 861–874, Jun. 2006. |
| [73] | J. Bergstra, D. Yamins, and D. D. Cox, "Making a science of model search: Hyperparameter optimization in hundreds of dimensions for vision architectures," in Proc. 30th Int. Conf. Mach. Learn., 2013, pp. 115–123. |
| [74] | M. Feurer and F. Hutter, "Hyperparameter optimization," in Automated Machine Learning: Methods, Systems, Challenges, F. Hutter, L. Kotthoff, and J. Vanschoren, Eds. Cham, Switzerland: Springer, 2019, pp. 3–33. |
| [75] | H. Wang and A. Banerjee, "Online alternating direction method," in Proc. 29th Int. Conf. Mach. Learn., 2012, pp. 1119–1126. |
| [76] | Y. Wang, D. Yin, L. Jie, P. Wang, M. Yamada, Y. Chang, and Q. Mei, "Beyond ranking: Optimizing whole-page presentation," in Proc. 9th ACM Int. Conf. Web Search Data Mining, 2016, pp. 103–112. |
| [77] | A. Graves, "Generating sequences with recurrent neural networks," arXiv:1308.0850, 2013. |
| [78] | I. Sutskever, O. Vinyals, and Q. V. Le, "Sequence to sequence learning with neural networks," in Proc. Adv. Neural Inf. Process. Syst., 2014, pp. 3104–3112. |
| [79] | K. Cho et al., "Learning phrase representations using RNN encoder-decoder for statistical machine translation," in Proc. Conf. Empirical Methods Natural Lang. Process., 2014, pp. 1724–1734. |
| [80] | S. Ruder, "An overview of gradient descent optimization algorithms," arXiv:1609.04747,2016. |
| [81] | N. Srivastava, G. Hinton, A. Krizhevsky, I. Sutskever, and R. Salakhutdinov, "Dropout: A simple way to prevent neural networks from overfitting," J. Mach. Learn. Res., vol. 15, no. 1, pp. 1929–1958, Jan. 2014. |
| [82] | S. Ioffe and C. Szegedy, "Batch normalization: Accelerating deep network training by reducing internal covariate shift," in Proc. 32nd Int. Conf. Mach. Learn., 2015, pp. 448–456. |
| [83] | D. Bahdanau, K. Cho, and Y. Bengio, "Neural machine translation by jointly learning to align and translate," in Proc. 3rd Int. Conf. Learn. Represent., 2015, pp. 1–15. |
| [84] | Z. Yang, D. Yang, C. Dyer, X. He, A. Smola, and E. Hovy, "Hierarchical attention networks for document classification," in Proc. Conf. North Amer. Chapter Assoc. Comput. Linguistics: Human Lang. Technol., 2016, pp. 1480–1489. |
| [85] | J. Devlin, M.-W. Chang, K. Lee, and K. Toutanova, "BERT: Pre-training of deep bidirectional transformers for language understanding," in Proc. Conf. North Amer. Chapter Assoc. Comput. Linguistics: Human Lang. Technol., 2019, pp. 4171–4186. |
| [86] | T. B. Brown et al., "Language models are few-shot learners," in Proc. Adv. Neural Inf. Process. Syst., 2020, pp. 1877–1901. |
| [87] | A. Radford et al., "Learning transferable visual models from natural language supervision," in Proc. 38th Int. Conf. Mach. Learn., 2021, pp. 8748–8763. |
| [88] | M. Bojarski et al., "End to end learning for self-driving cars," arXiv:1604.07316, 2016. |
| [88] | V. Mnih et al., "Human-level control through deep reinforcement learning," Nature, vol. 518, no. 7540, pp. 529–533, Feb. 2015. |
| [89] | D. Silver et al., "Mastering the game of Go with deep neural networks and tree search," Nature, vol. 529, no. 7587, pp. 484–489, Jan. 2016. |

## SHAPE REFERENCES

|  |  |
| --- | --- |
| [1] | " BP-NN model" Yinlong Liu and Jinze Li , 2022. https://www.mdpi.com/2227-9717/11/1/44 |
| [2] | Cloudio Owusu, “Geocoding Fundamentals and Associated Challenges” 2017. https://www.researchgate.net/publication/320760208\_Geocoding\_Fundamentals\_and\_Associated\_Challenges |
| [3] | Y. Lv, Y. Duan, W. Kang, Z. Li, and F. Y. Wang, “Traffic flow prediction with big data: A deep learning approach,” IEEE Transactions on Intelligent Transportation Systems, vol. 16, no. 2, pp. 865–873, Apr. 2015. |
| [4] | Code Block For Charge Stations |
| [5] | Part of the Code Block that analyse traffic density |
| [6] | Part of the Code Block That Makes Real Time Analysis |
| [7] | Part of the Code Block That Makes Energy Prediction |
| [8] | EV Car Estimation System Files |
| [9] | Traffic Control System |
| [10] | T. Ahmad and H. Chen, “Short and medium-term forecasting of cooling and heating load demand in building environment with data-driven approaches,” Energy and Buildings, vol. 166, pp. 460–476, Jun. 2018. |
| [11] | M. Moradzadeh and A. Khodaei, “An integrated approach for optimal siting and sizing of electric vehicle charging stations,” IEEE Transactions on Smart Grid, vol. 9, no. 5, pp. 4390–4399, Sept. 2018. |
| [12] | P. Neis, D. Zielstra, and A. Zipf, “The street network evolution of crowdsourced maps: OpenStreetMap in Germany 2007–2011,” Future Internet, vol. 4, no. 1, pp. 1–21, Mar. 2012. |
| [13] | S. Deb, K. Tammi, K. Kalita, and P. Mahanta, “Review of recent trends in charging infrastructure planning for electric vehicles,” Wiley Interdisciplinary Reviews: Energy and Environment, vol. 7, no. 6, p. e306, Nov. 2018. |
| [14] | C. Huang, Q. Pan, H. Zhang, and H. Wang, “A review on big data-based machine learning for smart traffic systems,” Information Fusion, vol. 66, pp. 17–33, Dec. 2020. |

## TABLE REFERENCES

|  |  |
| --- | --- |
| [1] | T. Ahmad and H. Chen, “Short and medium-term forecasting of cooling and heating load demand in building environment with data-driven approaches,” Energy and Buildings, vol. 166, pp. 460–476, Jun. 2018. |
| [2] | M. Moradzadeh and A. Khodaei, “An integrated approach for optimal siting and sizing of electric vehicle charging stations,” IEEE Transactions on Smart Grid, vol. 9, no. 5, pp. 4390–4399, Sept. 2018. |
| [3] | Y. Lv, Y. Duan, W. Kang, Z. Li, and F. Y. Wang, “Traffic flow prediction with big data: A deep learning approach,” IEEE Transactions on Intelligent Transportation Systems, vol. 16, no. 2, pp. 865–873, Apr. 2015. |
| [4] | S. Makridakis, E. Spiliotis, and V. Assimakopoulos, “Statistical and machine learning forecasting methods: Concerns and ways forward,” PLOS ONE, vol. 13, no. 3, p. e0194889, Mar. 2018. |
| [5] | J. W. Taylor, “Triple seasonal methods for short-term electricity demand forecasting,” European Journal of Operational Research, vol. 204, no. 1, pp. 139–152, Jan. 2010. |
| [6] | T. Chen and C. Guestrin, “XGBoost: A scalable tree boosting system,” in Proc. 22nd ACM SIGKDD Int. Conf. Knowledge Discovery Data Mining, 2016, pp. 785–794. |
| [7] | Y. Zheng, L. Capra, O. Wolfson, and H. Yang, “Urban computing: Concepts, methodologies, and applications,” ACM Transactions on Intelligent Systems and Technology (TIST), vol. 5, no. 3, pp. 1–55, Sept. 2014. |